This code takes data from the combined odometer/LiDAR position finding system and stores it in a manner readily legible to the intersection-finding code.

To use it properly, simply start up the robot’s systems, navigate to the folder containing the program, and run:

```

chmod +x get\_live\_combined.sh

./get\_live\_combined.sh

```